| ApossC SDK V01.15

SDK_Miscellaneous_IO.mh
Go to the documentation of this file.
1
8 #pragma once
9
10 // Declaration of the functions
11 long sdkSetupPwmGenerator_UserParamMode(long userParam, long digOutPWM,long frequency, long cycleRange, long polarity);
12 long sdkSetupPwmGenerator_AxisModeVel(long axisNo, long digOutEnable, long digOutPWM, long frequency, long cycleRange, long polarity);
13 long sdkScaleAnalogInput(long analogInputNo, long minVoltage, long maxVoltage,long offsetVoltage, long minValue, long maxValue);
sdkScaleAnalogInput
long sdkScaleAnalogInput(long analogInputNo, long minVoltage, long maxVoltage, long offsetVoltage, long minValue, long maxValue)
Scaling of an analog input with user units.
Definition: SDK_Miscellaneous_IO.mc:127
sdkSetupPwmGenerator_UserParamMode
long sdkSetupPwmGenerator_UserParamMode(long userParam, long digOutPWM, long frequency, long cycleRange, long polarity)
Setting up a PWM output with a user parameter as input source.
Definition: SDK_Miscellaneous_IO.mc:33
sdkSetupPwmGenerator_AxisModeVel
long sdkSetupPwmGenerator_AxisModeVel(long axisNo, long digOutEnable, long digOutPWM, long frequency, long cycleRange, long polarity)
Setting up a PWM output with a virtual amplifier as input source.
Definition: SDK_Miscellaneous_IO.mc:74

Data Sheets | Released Software | Software Manuals | Hardware Manuals | Maxon Shop

Maxon Support Center